Spectrum Camera Solutions D210-A-2.0CH5APTZDP36-BD Explosion-Proof 2MP PTZ 360° Network Camera
Certified (cFMus, ATEX, IECEx, INMETRO, UKEX/UKCA and PESO) for use in potentially combustible environments, this 2MP PTZ camera is a cost-effective, high-performance Explosion-Proof camera with an Image Rate of 1080p @ 60 fps and 36x zoom. It provides wide area coverage, high speed tracking and long-range details with 360° views to monitor large areas. Advanced low-light technology to capture low-light images with more saturated colors and sharper images of moving objects.
• 2MP camera with 32x zoom
• 1080p @ 60fps
• Advanced low-light technology
• Built-in Analytics
• Support for H.264, H.265 and MJPEG
• cFMus, ATEX, IECEx, INMETRO, UKEX/UKCA and PESO approved
• Class I II III Division 1 Gr B,C,D,E,F,G; II 2 G Ex db IIB+H2 Gb II 2 D Ex tb IIIC T85°C Db
• Temperature range: -20°C to +55°C 
• Made in Houston, Texas.

The main unit shall be backed by a five-year manufacturer’s warranty.
The product, including all its components, shall not contain any added PVC.
The contractor or designated subcontractor shall submit credentials of completed manufacturer certification, verified by a third-party organization, as proof of the knowledge.
Casing
A = Aluminum casing powder coated red

Explosion-proof Certifications
USA (Divisions):
Class I Division 1 Groups B,C,D T6, type 4X, IP66/67
Class II/III, Division 1, Groups E,F,G T6
Ta = -20°C to +55°C
Certificate: FM17US0156X
USA and Canada (Zones):
Class I, Zone 1, AEx/Ex db IIB+H2 T6 Gb Ta -20°C to +55°C, Type 4X, IP66/67
Zone 21, AEx/Ex tb IIIC T85 °C Db Ta = -20°C to +55°C, Type 4X, IP66/67
Certificate: FM17US0156X and FM18CA0103X
ATEX:
II 2 G Ex db IIB+H2 T6 Gb Ta = -20°C to +55°C, IP66/67
II 2 D Ex tb IIIC T85°C Db Ta = -20°C to +55°C, IP66/67
Certificate: FM18ATEX0057X
IECEx:
Ex db IIB+H2 T6 Gb Ta = -20°C to +55°C, IP66/67
Ex tb IIIC T85°C Db Ta = -20°C to +55°C, IP66/67
Certificate: FMG 18.0020X
INMETRO:
Ex db IIB+H2 T6 Gb Ta = -20°C to +55°C, IP66/67
Ex tb IIIC Db T85 °C Ta = -20°C to +55°C, IP66/67
Certificate number: NCC 20.0083 X
PESO:
Ex db IIB+H2 T6 Gb Ta = -20°C to +55°C, IP66/67
Ex tb IIIC T85 °C Db Ta = -20°C to +55°C, IP66/67
Certificate: FMG 18.0020X
Approval No: A/P/HQ/MH/104/7899 (P578984)
Approvals
Hazardous Area
FM3600, FM3615, ANSI/ISA/EN/IEC/CAN/CSA-C22.2 60079-0, ANSI/UL/EN/IEC/CAN/CSA-C22.2 60079-1, ANSI/UL/IEN/EC/CAN/CSA-C22.2 60079-31
EMC
EN 55032 Class A, EN 50121-4, IEC 62236-4, EN 55024, EN 61000-6-1, EN 61000-6-2, FCC Part 15 Subpart B Class A, ICES-003 Class A, VCCI Class A, RCM AS/NZS CISPR 32 Class A, KC KN32 Class A, KC KN35
Safety
IEC/EN/UL 62368-1, IEC/EN/UL 60950-22, IS 13252
Environment
IEC 60068-2-1, IEC 60068-2-2, IEC 60068-2-6, IEC 60068-2-14, IEC 60068-2-27, IEC 60068-2-78, IEC/EN 60529, IP66/IP67, IEC/EN 62262 IK10, NEMA 250 Type 4X, NEMA TS 2 (2.2.7-2.2.9)
Network
NIST SP500-267
Image sensor
1/2.8” progressive scan CMOS
Minimum illumination
Color: 0.1 lux at F1.6
B/W: 0.03 lux at F1.6

Lens
Varifocal, 4.3-129mm, F1.6 - 4.7, autofocus
Angle of view: 63.7°- 1.9°
Zoom: 36x (with image stabilization off), 30x (with image stabilization on)
Day and night
Automatic, Manual
Shutter speed
Automatic, Manual (1/1 to 1/10,000 sec) 
Video compression
H.264 HDSM SmartCodec
H.265 HDSM SmartCodec
Motion JPEG
Video streaming
Multi-streams in H.264, H.265 and Motion JPEG
Resolution
1920 (H) x 1080 (V)

Frame rate
Up to 60 fps
Image settings
Motion detection, Iris control, Flicker control at 60/50Hz, White balance, Backlight compensation, up to 64, 3D privacy zones, 500 named presets, 10 named tours, up to 100x digital zoom, electronic image stabilization and digital defog.
Audio Input/Output
Line level input and output
Security
Password protection, HTTPS encryption, digest authentication, WS authentication, user access log, 802.1x port based authentication, FIPS 140-2 L1
Supported protocols
IPv4, IPv6, HTTP, HTTPS, SOAP, DNS, NTP, RTSP, RTCP, RTP, TCP, UDP, IGMP, ICMP, DHCP, ARP, ZeroConf.
Streaming protocols
RTP/UDP, RTP/UDP Multicast, RTP/RTSP/TCP, RTP/RTSP/HTTP/TCP, RTP/RTSP/HTTPS/TCP, HTTP
Application Programming Interface
ONVIF® compliance version 1.02, 2.00
ONVIF® Profile G, ONVIF® Profile S, and ONVIF® Profile T
Supported Analytics Events
•	Objects in Area – The event is triggered when the selected object type moves into the region of interest.
•	Objects Loitering – The event is triggered when the selected object type moves into the region of interest and then stays for an extended period of time.
•	Objects Crossing Beam – The event is triggered when the specified number of objects have crossed the directional beam that is configured over the camera’s field of view. The beam can be unidirectional or bidirectional.
•	Object Appears or Enters Area – The event is triggered by each object that enters the region of interest. This event can be used to count objects.
•	Object Not Present in Area – The event is triggered when no objects are present in the region of interest.
•	Objects Enter Area – The event is triggered when the specified number of objects have entered the region of interest.
•	Objects Leave Area – The event is triggered when the specified number of objects have left the region of interest.
•	Object Stops in Area – The event is triggered when an object moves into a prohibited area of travel.
•	Direction Violation – The event is triggered when an object moves into the prohibited direction of travel.
•	Tamper Detection – The event is triggered when the scene unexpectedly changes.
Supported Classifies Objects
•	Object Types in Outdoor Mode – Vehicle, sub-types: Car, Truck, Bicycle, Motorcycle, Bus, Person
•	Object Types in Indoor Mode – Person
Power
IEEE 802.3bt, 60 WPoE
Connectors
100BASE-TX
RJ45
Storage
2 × microSD/microSDHC/microSDXC slot – minimum class 6; class 10/UHS-1 or better recommended. Currently one of the two SD card slots is available for onboard storage.
Operating conditions
-20°C to +55°C 
Storage conditions
-10 °C to +70 °C (14 °F to 158 °F)
Humidity 0–95% RH (non-condensing)
Dimensions
Height: 404 mm (15.9 in)
ø 218.44 mm (8.6 in)
Weight
14 kg (32 lbs)