Spectrum Camera Solutions D101-X-M4328-P-BD Explosion-Proof 180° and 360° 12MP Fisheye Camera
Certified (cFMus, ATEX, IECEx, INMETRO, UKEX/UKCA and PESO) for use in potentially combustible environments, this 12MP fisheye, deep learning camera can deliver 180° and 360° panoramic overviews as well as a variety of de-warped views with no blind spots. It supports day/night functionality for improved sensitivity in poor light, and advanced WDR imaging technology provides clarity when there's both dark and light areas in the scene. Furthermore, it features reduced bandwidth and storage needs technology and a powerful capacity for analytics. It offers powerful artificial intelligence and deep learning analytics. This product is delivered factory focused and features digital roll functionality for easy installation. Made from environmentally friendly materials, it’s re-paintable to blend in with any surroundings and there’s black, vandal-resistant and smoke-detector casings available as accessories.
• 180°/360° panoramic views at up to 30 fps
• Advanced low-light technology and Forensic WDR imaging
• Small and discreet design
• Zipstream support H.264 and H.265
• Support for digital PTZ views
• Environmentally friendly materials
• Temperature Range: 0°C to +40°C (32°F to 104°F)
• cFMus, ATEX, IECEx, INMETRO, UKEX/UKCA and PESO approved
• Class I II III Division 1 Gr B,C,D,E,F,G; II 2 G Ex db IIB+H2 Gb II 2 D Ex tb IIIC T85°C Db
• Made in Houston, Texas.

The main unit shall be backed by a five-year manufacturer warranty.
The product, including all its components, shall not contain any added PVC.
The contractor or designated subcontractor shall submit credentials of completed manufacturer certification, verified by a third-party organization, as proof of the knowledge.
Casing (X)
A = Aluminum casing powder coated red
S = Stainless Steel casing 316L

Explosion-proof Certifications
USA (Divisions):
Class I Division 1 Groups B,C,D T6, type 4X, IP66/67
Class II/III, Division 1, Groups E,F,G T6
Ta = 0°C to +40°C
Certificate: FM17US0156X
USA and Canada (Zones):
Class I, Zone 1, AEx/Ex db IIB+H2 T6 Gb Ta 0°C to +40°C, Type 4X, IP66/67
Zone 21, AEx/Ex tb IIIC T85 °C Db Ta = 0°C to +40°C, Type 4X, IP66/67
Certificate: FM17US0156X and FM18CA0103X
ATEX:
II 2 G Ex db IIB+H2 T6 Gb Ta = 0°C to +40°C, IP66/67
II 2 D Ex tb IIIC T85 °C Db Ta = 0°C to +40°C, IP66/67
Certificate: FM18ATEX0057X
IECEx:
Ex db IIB+H2 T6 Gb Ta = 0°C to +40°C, IP66/67
Ex tb IIIC T85 °C Db Ta = 0°C to +40°C, IP66/67
Certificate: FMG 18.0020X
INMETRO:
Ex db IIB+H2 T6 Gb Ta = 0°C to +40°C, IP66/67
Ex tb IIIC Db T85 °C Ta = 0°C to +40°C, IP66/67
Certificate number: NCC 20.0083 X
PESO:
Ex db IIB+H2 T6 Gb Ta = 0°C to +40°C, IP66/67
Ex tb IIIC T85 °C Db Ta = 0°C to +40°C, IP66/67
Certificate: FMG 18.0020X
Approval No: A/P/HQ/MH/104/7899 (P578984)
Approvals
Hazardous Area
FM3600, FM3615, ANSI/ISA/EN/IEC/CAN/CSA-C22.2 60079-0, ANSI/UL/EN/IEC/CAN/CSA-C22.2 60079-1, ANSI/UL/IEN/EC/CAN/CSA-C22.2 60079-31
EMC
EN 55032 Class A, EN 50121-4, IEC 62236-4, EN 55024, EN 61000-6-1, EN 61000-6-2, FCC Part 15 Subpart B Class A, ICES-003 Class A, VCCI Class A, RCM AS/NZS CISPR 32 Class A, KC KN32 Class A, KC KN35
Safety
IEC/EN/UL 60950-22, IEC/EN/UL 62368-1, IS 13252 
Environment
IEC 60068-2-1, IEC 60068-2-2, IEC 60068-2-6, IEC 60068-2-14, IEC 60068-2-27, IEC 60068-2-78, IEC 60529 IP66/IP67, IEC/EN 62262 IK10, NEMA 250 Type 4X, NEMA TS 2 (2.2.7-2.2.9)
Network
NIST SP500-267
Image sensor
1/2.3” progressive scan RGB CMOS
Lens
1.2 mm, F2.2
Horizontal field of view: 182°
Vertical field of view: 182°
Fixed iris, Fixed focus, IR corrected

Day and night
Automatically removable infrared-cut filter
Minimum illumination
Color: 0.19 lux at 50 IRE, F2.2
B/W: 0.04 lux at 50 IRE, F2.2
Shutter speed
1/8100 s to ½ s
Camera angle adjustment
Digital roll: +/- 180°
System on Chip model
Manufacturer’s own chipset
Memory
2048 MB RAM, 8192 MB Flash
Video compression
H.264 (MPEG-4 Part 10/AVC) Baseline, Main and High Profiles
H.265 (MPEG-H Part 2/HEVC) Main Profile
Motion JPEG
Resolution
Overview: 2992x2992 to 160x160 (1:1)
Panorama: 3840x2160 to 192x72 (8:3, 16:9 or 32:9)
Double panorama: 3584x2688 to 384x288 (4:3 or 16:9)
Quad view: 3584x2688 to 384x288 (4:3 or 16:9)
View area 1-4: 2048x1536 to 256x144 (4:3 or 16:9)
Corner left/right: 3200x1600 to 192x72 (2:1 or 8:3)
Double corner: 2880x2880 to 384x288 (1:1 or 4:3)
Corridor: 2560x1920 to 256x144 (4:3 or 16:9)
Frame rate
360° overview only up to max resolution without WDR: 25/30 fps @ 50/60 Hz
360° overview and 4 de-warped views up to max resolution with WDR: up to 25/20 fps @ 50/60 Hz
Video streaming
Multiple, individually configurable streams in H.264, H.265 and Motion JPEG
Axis Zipstream technology in H.264 and H.265
Controllable frame rate and bandwidth
VBR/ABR/MBR H.264/H.265
Video streaming indicator
WDR
Forensic WDR: Up to 120 dB depending on scene
Noise Reduction
Spatial filter (2D noise reduction)
Temporal filter (3D noise reduction)

Image settings
Saturation, contrast, brightness, sharpness, local contrast, tone mapping, white balance, day/night threshold, exposure mode, exposure zones, compression, mirroring, dynamic text and image overlay and polygon privacy mask
Image processing
Axis Zipstream, Forensic WDR
Pan/Tilt/Zoom
Digital PTZ of view areas, digital PT of panorama, corner, corridor and quad views, preset positions, guard tours
Audio input/output
Audio features through portcast technology: two-way audio connectivity, voice enhancer
Supported protocols
IPv4, IPv6 USGv6, ICMPv4/ICMPv6, HTTP, HTTP/2, HTTPS, TLS, QoS Layer 3 DiffServ, FTP, SFTP, CIFS/SMB, SMTP, mDNS (Bonjour), UPnP®, SNMP v1/v2c/v3 (MIB-II), DNS/DNSv6, DDNS, NTP, NTS, RTSP, RTP, SRTP, TCP, UDP, IGMPv1/v2/v3, RTCP, ICMP, DHCPv4/v6, SSH, SSH, LLDP, CDP, MQTT v3.1.1, Syslog, Link-Local address (ZeroConf), IEEE 802.1X (EAP-TLS), IEEE 802.1AR
Application Programming Interface
Open API for software integration, including VAPIX®, metadata and Axis Camera Application Platform (ACAP). ACAP includes Native SDK and Computer Vision SDK.
One-Click cloud connection.
ONVIF® Profile G, ONVIF® Profile M, ONVIF® Profile S, and ONVIF® Profile T.
Support for Session Initial Protocol (SIP) for integration with Voice over IP (VoIP) systems, peer to peer or integrated with SIP/PBX
Event conditions
Device status: above operating temperature, above or below operating temperature, below operating temperature, within operating temperature, IP address removed, new IP address, network lost, system ready, live stream active
Edge storage: recording ongoing, storage disruption, storage health issues detected
I/O: manual trigger, virtual input
MQTT: subscribe
Scheduled and recurring: schedule
Video: average bitrate degradation, day-night mode, tampering
Event actions
Day-night mode
MQTT: publish
Notification: HTTP, HTTPS, TCP and email
Overlay text
Recordings: SD card and network share
SNMP traps: send, send while the rule is active
Status LED
Upload of images or video clips: FTP, SFTP, HTTP, HTTPS, network share and email
WDR mode
Built-in installation aids
Pixel counter, digital roll, level grid

Security
Password protection, IP address filtering, HTTPS encryption, IEEE 802.1X (EAP-TLS) network access control, digest authentication, user access log, centralized certificate management, brute force delay protection, signed firmware, secure boot
Object Analytics
Object classes: humans, vehicles (types: cars, buses, trucks, bikes)
Features: line crossing, object in area
Up to 10 scenarios
Metadata visualized with trajectories, color-coded bounding boxes and tables
Polygon include/exclude areas
ONVIF Motion Alarm event
Metadata
Object data: Classes: humans, faces, vehicles (types: cars, buses, trucks, bikes), license plates
Confidence, position
Event data: Producer reference, scenarios, trigger conditions
Applications
Included
AXIS Object Analytics, AXIS Video Motion Detection, active tampering alarm
Supported
Support for AXIS Camera Application Platform enabling installation of third-party applications
Power
Power 44-57 VDC, 6.49W
Operating conditions
0°C to +40°C (32°F to 104°F)
Humidity 10-100% RH (condensing)
Storage conditions
-40°C to 65°C (-40°F to 149°F)
Humidity 5-95% RH (non-condensing)
Dimensions
Height: 292mm (11.5 in)
ø 218mm (8.6 in)

Weight
A = 19lbs (8.61kg)
S = 47lbs (21.31kg)
Languages (Camera)
English, German, French, Spanish, Italian, Russian, Simplified Chinese, Japanese, Korean, Portuguese, Traditional Chinese