Spectrum Camera Solutions D101-X-P3818-BD Explosion-Proof Camera
Certified (cFMus, ATEX, IECEx, INMETRO, UKEX/UKCA and PESO) for use in potentially combustible environments, this camera delivers a 180º panoramic overview of extensive areas with ultra-high resolution images and incredible details up to 30 fps. With 13 MP resolution and seamless stitching of all three images, it offers 180° horizontal and 90° vertical coverage with no blind spots. Including a variety of mounting options, it’s also possible to mount two cameras back-to-back for a complete 360° overview, using a dual camera mount. Featuring edge-to-edge technology, it’s easy to add support for audio enabling you to listen in to transactions or incidents. Additionally, built-in cybersecurity features prevent unauthorized access and safeguard your system.
• 13 MP multisensor camera with one IP address
• 180° horizontal, 90° vertical coverage
• Seamlessly stitched images
• Support for audio input 
• Built-in cybersecurity features
• Temperature Range: -20°C to +50°C (-4°F to 122°F)
• cFMus, ATEX, IECEx, INMETRO, UKEX/UKCA and PESO approved
• Class I II III Division 1 Gr B,C,D,E,F,G; II 2 G Ex db IIB+H2 Gb II 2 D Ex tb IIIC T85°C Db
• Made in Houston, Texas.

The main unit shall be backed by a five-year manufacturer warranty.
The contractor or designated subcontractor shall submit credentials of completed manufacturer certification, verified by a third-party organization, as proof of the knowledge.
Casing (X)
A = Aluminum casing powder coated red
S = Stainless Steel casing 316L
Explosion-proof Certifications
USA (Divisions):
Class I Division 1 Groups B,C,D T6, type 4X, IP66/67
Class II/III, Division 1, Groups E,F,G T6
Ta = -20°C to +50°C
Certificate: FM17US0156X
USA and Canada (Zones):
Class I, Zone 1, AEx/Ex db IIB+H2 T6 Gb Ta -20°C to +50°C, Type 4X, IP66/67
Zone 21, AEx/Ex tb IIIC T85 °C Db Ta = -20°C to +50°C, Type 4X, IP66/67
Certificate: FM17US0156X and FM18CA0103X
ATEX:
II 2 G Ex db IIB+H2 T6 Gb Ta = -20°C to +50°C, IP66/67
II 2 D Ex tb IIIC T85 °C Db Ta = -20°C to +50°C, IP66/67
Certificate: FM18ATEX0057X
IECEx:
Ex db IIB+H2 T6 Gb Ta = -20°C to +50°C, IP66/67
Ex tb IIIC T85 °C Db Ta = -20°C to +50°C, IP66/67
Certificate: FMG 18.0020X
INMETRO:
Ex db IIB+H2 T6 Gb Ta = -20°C to +50°C, IP66/67
Ex tb IIIC Db T85 °C Ta = -20°C to +50°C, IP66/67
Certificate number: NCC 20.0083 X
PESO:
Ex db IIB+H2 T6 Gb Ta = -20°C to +50°C, IP66/67
Ex tb IIIC T85 °C Db Ta = -20°C to +50°C, IP66/67
Certificate: FMG 18.0020X
Approval No: A/P/HQ/MH/104/7899 (P578984)
Approvals
Hazardous Area
FM3600, FM3615, ANSI/ISA/EN/IEC/CAN/CSA-C22.2 60079-0, ANSI/UL/EN/IEC/CAN/CSA-C22.2 60079-1, ANSI/UL/IEN/EC/CAN/CSA-C22.2 60079-31
EMC
EAC, EN 55032 Class A, EN 55035, EN 50121-4, IEC 62236-4, EN 55024, EN 61000-6-1, EN 61000-6-2, FCC Part 15 Subpart B Class A, ICES-3(A)/NMB-3(A), VCCI Class A, RCM AS/NZS CISPR 32 Class A, KC KN32 Class A, KC KN35, CISPR 24, CISPR 35
Safety
IEC/EN/UL 60950-22, IEC/EN/UL 62368-1, CAN/CSA C22.2 No. 62368-1, CAN/CSA-C22.2 No. 60950-22, IS 13252
Environment
IEC 60068-2-1, IEC 60068-2-2, IEC 60068-2-6, IEC 60068-2-14, IEC 60068-2-27, IEC 60068-2-78, IEC/EN 60529 IP66/IP67, IEC/EN 62262 IK10, NEMA 250 Type 4X, NEMA TS 2 (2.2.7-2.2.9), MIL-STD-810H (Method 501.7, 502.7, 505.7, 506.6, 507.6, 509.7, 512.6)
Network
NIST SP500-267

Image sensor
3 x 5 MP 1/2.8” progressive scan RGB CMOS 
Lens
Fixed 3.2 mm, F2.0
Horizontal field of view: 180°
Vertical field of view: 90°

Day and night
Automatically removable infrared-cut filter
Minimum illumination
With advanced WDR imaging technology and low-light technology:
Color: 0.16 lux, F2.0
B/W: 0.05 lux, F2.0
Shutter speed
1/91000 to 1/25 s 
With WDR: 1/50000 to 1/25 s 
Camera angle adjustment
Pan +/- 180°
Tilt 0° to 50°
Roll +/- 5°
System on Chip model
Manufacturer’s own chipset (x2)
Memory
2048 MB RAM (x2), 512 MB Flash
Compute capabilities
Machine learning processing unit (MLPU)
Video compression
H.264 (MPEG-4 Part 10/AVC) Baseline, Main and High Profiles
H.265 (MPEG-H Part 2/HEVC) Main Profile
Motion JPEG
Resolution
5120x2560 (13.1 MP) to 608x128
Frame rate
13.1 MP @ 25/30 fps (50/60 Hz) WDR
Video streaming
13.1 MP: 1 configurable stream in H.264, H.265 and Motion JPEG in full frame rate
Controllable frame rate and bandwidth
VBR/ABR/MBR H.264/H.265
Image settings
Saturation, contrast, brightness, sharpness, advanced WDR imaging technology: up to 120 dB depending on scene, white balance, day/night threshold, exposure mode, compression, dynamic text and image overlay, orientation aid, exposure control, noise reduction, fine tuning of behavior at low light, polygon privacy masks
Audio streaming
Two-way audio via edge-to-edge technology
Audio input/output
External microphone input, line input, digital audio input, automatic gain control, network speaker pairing
Audio encoding
24bit LPCM, AAC-LC 8/16/32/48 kHz, G.711 PCM 8 kHz, G.726 ADPCM 8 kHz, Opus 8/16/48 kHz, 44.1 kHz ACC-LC, LPCM
Configurable bit rate
Security
Password protection, IP address filtering, HTTPS encryption, IEEE 802.1X (EAP-TLS) network access control, digest authentication, user access log, centralized certificate management, brute force delay protection, signed firmware, cryptographic compute module, Manufacturer's device ID, secure keystore (CC EAL4 certified), TPM (FIPS 140-2 certified)
Supported protocols
IPv4, IPv6 USGv6, ICMPv4/ICMPv6, HTTP, HTTP/2, HTTPS, TLS, QoS Layer 3 DiffServ, FTP, SFTP, CIFS/SMB, SMTP, mDNS (Bonjour), UPnP®, SNMP v1/v2c/v3 (MIB-II), DNS/DNSv6, DDNS, NTP, RTSP, RTP, TCP, UDP, IGMP, RTCP, ICMP, DHCPv4/v6, ARP, SOCKS, SSH, LLDP, CDP, MQTT, Syslog, Link-Local address (ZeroConf)
Application Programming Interface
Open API for software integration
ONVIF® Profile G, ONVIF® Profile M, ONVIF® Profile S and ONVIF® Profile T
Event conditions
Analytics, external input, supervised external input, edge storage events, virtual inputs through API
Audio: audio detection
Digital audio: digital signal contains metadata, digital signal as invalid sample rate, digital signal missing, digital signal ok
Device status: above operating temperature, above or below operating temperature, below operating temperature, fan failure, IP address removed, network lost, new IP address, shock detected, storage failure, system ready, within operating temperature, casing open, ring power overcurrent protection
Edge storage: recording ongoing, storage disruption, storage health issues detected
I/O: digital input, manual trigger, virtual input
MQTT subscribe
Scheduled and recurring: scheduled event
Video: live stream open, average bitrate degradation, day-night mode, tampering
Event actions
Day/night mode, overlay text, video recording to edge storage, pre- and post-alarm video buffering, send SNMP trap, play audio clipm I/O events, status LED events
File upload: FTP, SFTP, HTTP, HTTPS network share, email
MQTT publish
Notification: email, HTTP, HTTPS TCP
Data streaming
Event data
Built-in installation aids
Pixel counter, leveling guide
Applications
Included
fence guard, motion guard, loitering guard
video motion detection, active tampering alarm, audio detection
Supported
Support for enabling installation of third-party applications
Sustainability
PVC free, 20% recycled plastic
Power
Power over Ethernet (PoE) IEEE 802.3at Type 2 Class 4
Typical 11 W, max 18 W
Connectors
Shielded RJ45 1000BASE-T
Terminal block for two configurable supervised inputs/digital outputs (12 V DC output, max load 50 mA), 3.5 mm analog/digital mic/line in
Storage
Support for microSD/microSDHC/microSDXC card
Support for SD card encryption
Support for recording to network-attached storage (NAS)
Operating conditions
-20°C to +50°C (-4°F to 122°F)
Storage conditions
-40°C to 65°C (-40°F to 149°F)
Humidity 5-95% RH (non-condensing)
Dimensions
Height: 292mm (11.5 in)
ø 218mm (8.6 in)

Weight
A = 19lbs (8.61kg)
S = 47lbs (21.31kg)
Languages (Camera)
English, German, French, Spanish, Italian, Russian, Simplified Chinese, Japanese, Korean, Portuguese, Traditional Chinese