Spectrum Camera Solutions D201-X-Q6075-E-BD Explosion-Protected PTZ Camera
Certified (cFMus, ATEX, IECEx, INMETRO, UKEX/UKCA and PESO) for use in potentially combustible environments, this camera offers HDTV 1080p and 40x optical zoom for great overview and excellent detail. Featuring advanced low-light technology, it captures images with more realistic and saturated colors and sharper images of moving objects. It includes autotracking with click and track functionality for active object tracking, and orientation aid with support for dynamic overlays for quick orientation. Built-in cybersecurity features such as signed firmware and secure boot ensure the integrity and authenticity of the firmware. Furthermore, reduced bandwidth and storage needs technology with support for H.264/H.265 significantly lowers bandwidth and storage requirements.
• HDTV 1080p at 50/60 fps, with 40x optical zoom
• Advanced low-light technology
• Autotracking and orientation aid
• TPM, FIPS 140–2 level 2 certified
• Temperature Range: -20°C to +50°C (-4°F to 122°F)
• cFMus, ATEX, IECEx, INMETRO, UKEX/UKCA and PESO approved
• Class I II III Division 1 Gr B,C,D,E,F,G; II 2 G Ex db IIB+H2 Gb II 2 D Ex tb IIIC T85°C Db
• Made in Houston, Texas.

The embedded analytics shall be backed by free support within warranty period.
The main unit shall be backed by a five-year manufacturer warranty.
The contractor or designated subcontractor shall submit credentials of completed manufacturer certification, verified by a third-party organization, as proof of the knowledge.

Casing (X)
A = Aluminum casing powder coated red
S = Stainless Steel casing 316L

Explosion-proof Certifications
USA (Divisions):
Class I Division 1 Groups B,C,D T6, type 4X, IP66/67
Class II/III, Division 1, Groups E,F,G T6
Ta = -20 °C to +50°C
Certificate: FM17US0156X
USA and Canada (Zones):
Class I, Zone 1, AEx/Ex db IIB+H2 T6 Gb Ta -20°C to +50°C, Type 4X, IP66/67
Zone 21, AEx/Ex tb IIIC T85 °C Db Ta = -20°C to +50°C, Type 4X, IP66/67
Certificate: FM17US0156X and FM18CA0103X
ATEX:
II 2 G Ex db IIB+H2 T6 Gb Ta = -20°C to +50°C, IP66/67
II 2 D Ex tb IIIC T85 °C Db Ta = -20°C to +50°C, IP66/67
Certificate: FM18ATEX0057X
IECEx:
Ex db IIB+H2 T6 Gb Ta = -20°C to +50°C, IP66/67
Ex tb IIIC T85 °C Db Ta = -20°C to +50°C, IP66/67
Certificate: FMG 18.0020X
INMETRO:
Ex db IIB+H2 T6 Gb Ta = -20°C to +50°C, IP66/67
Ex tb IIIC Db T85 °C Ta = -20°C to +50°C, IP66/67
Certificate number: NCC 20.0083 X
PESO:
Ex db IIB+H2 T6 Gb Ta = -20°C to +50°C, IP66/67
Ex tb IIIC T85 °C Db Ta = -20°C to +50°C, IP66/67
Certificate: FMG 18.0020X
Approval No: A/P/HQ/MH/104/7899 (P578984)
Approvals
Hazardous Area
FM3600, FM3615, ANSI/ISA/EN/IEC/CAN/CSA-C22.2 60079-0, ANSI/UL/EN/IEC/CAN/CSA-C22.2 60079-1, ANSI/UL/IEN/EC/CAN/CSA-C22.2 60079-31
EMC
EN 55032 Class A, EN 55024, EN 61000-3-2, EN 61000-3-3, EN 61000-6-2, FCC Part 15 Subpart B Class A, ICES-003 Class A, VCCI Class A, RCM AS/NZS CISPR 32 Class A
Safety
IEC/EN/UL 60950-1, IEC/EN/UL 60950-22, CAN/CSA-C22.2 No. 60950-22, EN 62368-1:2014/A11:2017, EN 60950-22:2017, IEC 62368-1:2014, IEC 60950-22, UL 62368-1:2014, UL 60950-22:2017, CAN/CSA C22.2 No.62368-1-14, CSA CAN/CSA C22.2 No. 60950-22-17
Environment
ANSI/IEC/CAN/CSA-C22.2 60529 IP66/67, NEMA 250 Type 4X
Network
NIST SP500-267
Explosion
ANSI/ISA/EN/IEC/CAN/CSA-C22.2 60079-0, ANSI/UL/EN/IEC/CAN/CSA-C22.2 60079-1, ANSI/UL/IEN/EC/CAN/CSA-C22.2 60079-31
Image sensor
1/2.8” progressive scan RGB CMOS

Lens
4.25-170 mm, F1.6-4.95
Horizontal field of view: 65.1°-2.0° (1080p)
Vertical field of view: 39.1°-1.18° (1080p)
Autofocus, auto-iris
Day and night
Automatically removable infrared-cut filter
Minimum illumination
Color: 0.1 lux at 30 IRE, F1.6
B/W: 0.002 lux at 30 IRE, F1.6
Color: 0.15 lux at 50 IRE, F1.6
B/W: 0.003 lux at 50 IRE, F1.6
Shutter speed
1/11000 s to 1/3 s
Pan/Tilt/Zoom
Pan: 360° endless, 0.05°–450°/s
Tilt: 220°, 0.05°–450°/s
Zoom: 40x optical, 12x digital, Total 480x zoom
E-flip, 256 preset positions, tour recording (max 10, max duration 16 minutes each), guard tour (max 100), control queue, on-screen directional indicator, orientation aid PTZ, set new pan 0°, adjustable zoom speed, focus recall
Model
Manufacturer’s own chipset
Memory
1024 MB RAM, 512 MB Flash
Video compression
H.264 (MPEG-4 Part 10/AVC) Baseline, Main and High Profiles
H.265 (MPEG-H Part 2/HEVC) Main Profile
Motion JPEG
Resolution
HDTV 1080p 1920x1080 to 320x180
Frame rate
Up to 50/60 fps (50/60 Hz) in HDTV 1080p
Video streaming
Multiple, individually configurable streams in H.264, H.265 and Motion JPEG

Controllable frame rate and bandwidth
VBR/ABR/MBR H.264 and H.265

Image settings
Manual shutter time, compression, color, brightness, sharpness, WDR: up to 120 dB depending on scene, white balance, exposure control, exposure zones, fine tuning of behavior at low light, rotation: 0°, 180°, dynamic text and image overlay, polygon privacy masks, image freeze on PTZ, automatic defog, backlight compensation, highlight compensation
Scene profiles: forensic, indoor, outdoor, traffic overview
Security
Password protection, IP address filtering, HTTPS encryption, IEEE 802.1x (EAP-TLS) network access control, digest authentication, user access log, centralized certificate management, brute force delay protection, signed firmware, secure boot, protection of cryptographic keys with FIPS 140-2 certified TPM 2.0 module
Supported protocols
IPv4, IPv6 USGv6, ICMPv4/ICMPv6, HTTP, HTTPS, HTTP/2, SSL/TLS, QoS Layer 3 DiffServ, FTP, SFTP, CIFS/SMB, SMTP, mDNS (Bonjour), UPnP®, SNMP v1/v2c/v3 (MIB-II), DNS/DNSv6, DDNS, NTP, RTSP, RTP, SRTP, TCP, UDP, IGMP, RTCP, ICMP, DHCPv4/v6, ARP, SOCKS, SSH, NTCIP, LLDP, CDP, MQTT v3.1.1, Syslog, Link-Local address (ZeroConf)
Application Programming Interface
Open API for software integration

ONVIF® Profile G, ONVIF® Profile M, ONVIF® Profile S and ONVIF® Profile T
Event conditions
Device status: above operating temperature, above or below operating temperature, below operating temperature, fan failure, IP address removed, network lost, new IP address, shock detected, storage failure, system ready, within operating temperature
Edge storage: recording ongoing, storage disruption
I/O: manual trigger, virtual input
MQTT subscribe
PTZ: PTZ malfunctioning, PTZ movement, PTZ preset position reached, PTZ ready
Scheduled and recurring: scheduled event
Video: live stream open
Event actions
Day/night mode, overlay text, video recording to edge storage, pre- and post-alarm video buffering, send SNMP trap
PTZ: PTZ preset, start/stop guard tour
File upload via FTP, SFTP, HTTP, HTTPS network share and email
Notification via email, HTTP, HTTPS and TCP
MQTT publish
Data streaming
Event data
Built-in installation aids
Pixel counter, leveling guide
Applications
Included
motion guard, fence guard, loitering guard, autotracking 2, active gatekeeper 
Basic analytics (not to be compared with third-party analytics): object removed, enter/exit detector, object counter
Support for enabling installation of third-party applications
Sustainability
PVC free
Power
High PoE 60 W SFP midspan: 100–240 V AC, max 66.1 W
Camera consumption: typical 14 W, max 51 W
Connectors
8-position terminal block for PoE + ground, one M20 conduit entry
Storage
Pre-installed 128 GB surveillance grade microSDXC card
Support for SD card encryption (AES-XTS-Plain64 256bit)
Support for recording to network-attached storage (NAS)
Operating conditions
-20°C to +50°C (-4°F to 122°F)
intelligent camera heating technology: Start-up at -20°C 
Humidity 10–100% RH (condensing)
Storage conditions
-40°C to 65°C (-40°F to 149°F)
Dimensions
Height: 404mm (15.9 in)
ø 218mm (8.6 in)
Weight
A = 32lbs (14 kg)
S = 68 lb (28 kg)
Languages (Camera)
English, German, French, Spanish, Italian, Russian, Simplified Chinese, Japanese, Korean, Portuguese, Traditional Chinese